| Network Key Configuration
| Enter the appropriate network key and click "Next". There are some rules for each security method.
| Open System/Shared Key with WEP This key is a 64-bit or 128-bit value that must be entered in an ASCII or hexadecimal format.

- 64 (40) bit ASCII:
  Uses 5 text characters e.g. "WSLAN" (this is case sensitive).
- 64 (40) bit hexadecimal:
  Uses 10 digits of hexadecimal data e.g. "71f2234aba".
- 128 (104) bit ASCII:
  Uses 13 text characters e.g. "Wirelesscomms" (this is case sensitive).
- 128 (104) bit hexadecimal:
  Uses 26 digits of hexadecimal data e.g. "71f2234ab56cd709e5412aa2ba".

WPA-PSK/WPA2-PSK and TKIP or AES
Uses a Pre-Shared Key (PSK) that is 8 or more characters in length, up to a maximum of 63 characters.