## Specifications

This chapter guides you about this machine’s specifications such as various features.

This chapter include:

- Hardware specifications

- Environmental specifications

- Electrical specifications

- Print media specifications

## Hardware specifications

Item | Description
--- | ---
Dimensions | Height | e-STUDIO220S: 275.8 mm (10.9 inches) e-STUDIO221S: 318.9 mm (12.6 inches)
Depth | e-STUDIO220S: 409 mm (16.1 inches) e-STUDIO221S: 415.4 mm (16.4 inches)
Width | e-STUDIO220S: 416 mm (16.4 inches) e-STUDIO221S: 416 mm (16.4 inches)
Weight | Machine with consumables | e-STUDIO220S: 10.59 Kg (23.35 lbs) e-STUDIO221S: 11.55 Kg (25.46 lbs)
Package weight | Paper | e-STUDIO220S: 2.13 Kg (4.7 lbs) e-STUDIO221S: 2.29 Kg (5.05 lbs)
Plastic | e-STUDIO220S: 0.62 Kg (1.37 lbs) e-STUDIO221S: 0.49 Kg (1.07 lbs)

## Environmental specifications

Item | Description
--- | ---
Noise Level[a] | Ready mode | 26 dB(A)
Printing mode | 50 dB(A)
Copying mode (scanner glass) | 50 dB(A)
Copying mode (document feeder) | 52 dB(A)
Temperature | Operation | 10 to 32 °C (50 to 90 °F)
Storage | 10 to 32 °C (50 to 90 °F)
Humidity | Operation | 20 to 80% RH
Storage | 20 to 80% RH
[a] Sound Pressure Level, ISO 7779. Configuration tested: machine basic installation, A4 paper, simplex printing.

## Electrical specifications

Power requirements are based on the country/region where the device is sold. Do not convert operating voltages. Doing so might damage the device and void the product warranty.

Item | Description
--- | ---
Power rating [a] | 220 volt models | AC 220 - 240 V
Power consumption | Average operating mode | Less than 370 W
Ready mode | Less than 45 W
Power save mode | Less than 10 W
Power off mode | Less than 1 W
[a] See the rating label on the machine for the correct voltage, frequency (hertz) and type of current for your machine.

## Print media specifications

Type | Size | Dimensions | Print media weight[a]/Capacity[b]
--- | --- | --- | ---
Tray1 | Manual tray
Plain paper | Letter | 216 x 279 mm (8.50 x 11.00 inches) | 60 to 120 g/m2 (16 to 32 lb bond) 250 sheets of 80g/m2 (20 lb bond) | 60 to 163 g/m2 (16 to 43 lb bond) 1 sheet stacking
Legal | 216 x 356 mm (8.50 x 14.00 inches)
US Folio | 216 x 330 mm (8.50 x 13.00 inches)
A4 | 210 x 297 mm (8.27 x 11.69 inches)
Oficio | 216 x 343 mm (8.50 x 13.50 inches)
JIS B5 | 182 x 257 mm (7.17 x 10.12 inches) | 60 to 90 g/m2 (16 to 24 lb bond) 150 sheets of 80 g/m2 (20 lb bond)
ISO B5 | 176 x 250 mm (6.93 x 9.84 inches)
Executive | 184 x 267 mm (7.25 x 10.50 inches)
A5 | 148 x 210 mm (5.83 x 8.27 inches)
A6 | 105 x 148 mm (4.13 x 5.83 inches)
Envelope | Envelope Monarch | 98 x 191 mm (3.87 x 7.50 inches) | Not available in tray1 | 75 to 90 g/m2 (20 to 24 lb bond) 1 sheet stacking
Envelope No. 10 | 105 x 241 mm (4.12 x 9.50 inches)
Envelope DL | 110 x 220 mm (4.33 x 8.66 inches)
Envelope C5 | 162 x 229 mm (6.38 x 9.02 inches)
Envelope C6 | 114 x 162 mm (4.49 x 6.38 inches)
Thick paper | Refer to the Plain paper section | Refer to the Plain paper section | 90 g/m2 (24 lb bond) | 90 g/m2 (24 lb bond) 1 sheet stacking
Thin paper | Refer to the Plain paper section | Refer to the Plain paper section | 60 to 70 g/m2 (16 to 19 lb bond) | 60 to 70 g/m2 (16 to 19 lb bond) 1 sheet stacking
Transparency | Refer to the Plain paper section | Refer to the Plain paper section | Not available in tray1 | 138 to 146 g/m2 (36.81 to 38.91 lb bond) 1 sheet stacking
Labels[c] | Letter, Legal, US Folio, A4, JIS B5, ISO B5, Executive, A5, Statement | Refer to the Plain paper section | Not available in tray1 | 120 to 150 g/m2 (32 to 40 lb bond) 1 sheet stacking
Card stock | Letter, Legal, US Folio, A4, JIS B5, ISO B5, Executive, A5, Statement, PostCard 4x6 | Refer to the Plain paper section | Not available in tray1 | 105 to 163 g/m2 (28 to 43 lb bond) 1 sheet stacking
Minimum size (custom) | 76 x 127 mm (3.00 x 5.00 inches) | 60 to 163 g/m2 (16 to 43 lb bond) |
Maximum size (custom) | 216 x 356 mm (8.50 x 14.02 inches)
[a] If media weight is over 120 g/m2 (32 lb), load a paper into the tray one by one. [b] Maximum capacity may differ depending on media weight, thickness, and environmental conditions. [c] Smoothness: 100 to 250 (sheffield).