## Supplies and accessories

This chapter provides information on purchasing supplies, accessories and maintenance parts available for your machine.

This chapter includes:

- How to purchase

- Available supplies

- Available maintenance parts

- Replacing the toner cartridge

- Checking replaceable’s lifespan

Available accessories may differ from country to country. Contact your sales representatives to obtain the list of available accessories.

## How to purchase

To order TOSHIBA TEC-authorized supplies, accessories and, maintenance parts, contact your local TOSHIBA TEC dealer or the retailer where you purchased your machine.

## Available supplies

When supplies reach their lifespan, you can order the following types of supplies for your machine:

Type | Average yield[a] | Part name
--- | --- | ---
High yield | Approx. 2,500 pages | T-2210C
[a] Declared yield value in accordance with ISO/IEC 19752.

To replace a toner cartridge see Replacing the toner cartridge.

Depending on the options and job mode used, the toner cartridge’s lifespan may differ.

You must purchase supplies, including toner cartridges, in the same country where you purchased your machine. Otherwise, supplies will be incompatible with your machine since the system configuration of these vary from country to country.

TOSHIBA TEC does not recommend using non-genuine TOSHIBA TEC toner cartridge such as refilled or remanufactured. TOSHIBA TEC cannot guarantee non-genuine TOSHIBA TEC toner cartridge's quality. Service or repair required as a result of using non-genuine TOSHIBA TEC toner cartridges will not be covered under the machine warranty.

## Available maintenance parts

To avoid print quality and paper feed problems resulting from worn parts and to maintain your machine in top working condition, the following parts will need to be replaced after printing the specified number of pages or when the life span of each item has expired.

parts | Average yield[a] | Part name
--- | --- | ---
Document feeder rubber pad | Approx. 20,000 pages | RMO ADF RUBBER
Transfer roller | Approx. 50,000 pages | ROLLER-TRANSFER
Fuser unit | Approx. 50,000 pages | FUSER
Pickup roller | Approx. 50,000 pages | ROLLER-PICK UP
Cassette unit | Approx. 50,000 pages | CASSETTE
[a] It will be affected by operating system used, computing performance, application software, connecting method, media type, media size and job complexity.

To purchase maintenance parts, contact the source where you bought the machine.

Replacing maintenance parts can be performed only by an authorized service provider, dealer, or the retailer where you bought the machine. The warranty does not cover the replacement of any maintenance parts after their lifespan.

## Replacing the toner cartridge

When a toner cartridge has reached its estimated cartridge life:

- End of life Replace new cart appears on the display.

- The machine stops printing. Incoming faxes are saved in memory.

At this stage, the toner cartridge needs to be replaced. Check the type of the toner cartridge for your machine (See Available supplies).

1. Open the front door.

2. Pull the toner cartridge out.

3. Take a new toner cartridge out of its package.

4. Remove the paper protecting the toner cartridge by pulling the packing tape.

5. Locate the sealing tape at the end of the toner cartridge. Carefully pull the tape completely out of the cartridge and discard it.

   The sealing tape should be longer than 60 cm (23.6 inches) when correctly removed. Holding the toner cartridge, pull the sealing tape straight to remove it from the cartridge. Be careful not to cut the tape. If this happens, you cannot use the toner cartridge. Refer to the helpful pictures on the cartridge wrapping paper.

6. Slowly shake the cartridge five or six times to distribute the toner evenly inside the cartridge. It will assure maximum copies per cartridge.

   If toner gets on your clothing, wipe it off with a dry cloth and wash clothing in cold water. Hot water sets toner into fabric.

   Do not touch the green underside of the toner cartridge. Use the handle on the cartridge to avoid touching this area.

7. Hold the toner cartridge by the handle and slowly insert the cartridge into the opening in the machine.

   Tabs on the sides of the cartridge and corresponding grooves within the machine will guide the cartridge into the correct position until it locks into place completely.

8. Close the front door. Make sure that the cover is securely closed.

## Checking replaceable’s lifespan

If you experience frequent paper jams or printing problems, check the number of pages the machine has printed. Replace the corresponding parts, if necessary.

1. Press Menu on the control panel.

2. Press the left/right arrow until System Setup appears and press OK.

3. Press the left/right arrow until Maintenance appears and press OK.

4. Press the left/right arrow until Supplies Life appears and press OK.

5. Press the left/right arrow until the item you want appears and press OK.

   - Supplies Info: Prints the supply information page.

   - Total: Displays the total number of pages printed.

   - ADF Scan: Displays the number of pages scanned using the ADF.

   - Platen Scan: Displays the number of pages scanned using the scanner glass.

6. Press Stop/Clear to return to ready mode.