Help on Port Settings - Ethernet page (Properties)

Port Settings - Ethernet
This page allows you to configure the settings for Ethernet.

Ethernet Settings
Select the transmission speed of Ethernet from the following.
This setting will become valid after rebooting the printer from WebAdmin services or manually switching it off and then on again.

- Auto
  Automatically detects and switches the Ethernet transmission speed and Duplex setting.
- 10Base-T Half-Duplex
  Select this to fix the transmission speed to 10Base-T Half-Duplex.
- 10Base-T Full-Duplex
  Select this to fix the transmission speed to 10Base-T Full-Duplex.
- 100Base-TX Half-Duplex
  Select this to fix the transmission speed to 100Base-TX Half-Duplex.
- 100Base-TX Full-Duplex
  Select this to fix the transmission speed to 100Base-TX Full-Duplex.

Current Ethernet Settings
Displays the current Ethernet transmission speed.

MAC Address
Displays the MAC address. This is a display-only item.

[Apply] button
[Undo] button