Help on Protocol Settings - Port9100 page (Properties)

Protocol Settings - Port9100
This page allows you to configure the settings for Port9100 (Raw Data Socket).

Port Number
Enter the Port9100 port number between 9000 and 9999. The default value is 9100.
This setting will become valid after rebooting the printer from WebAdmin services or manually switching it off and then on again.

Connection Time-Out
Set the connection time-out period of Port9100 protocol. If the reception of data stops before receiving the entire data, the Port9100 connection to the printer will time out after the time period set here. The time-out period can be set between 1 and 1,000 seconds.

IP Filter
Click this when controlling connections from certain IP addresses. When clicked, [IP Filter] page appears.

[Apply] button
[Undo] button