;; Realtek 10/100/1000 PCI-E NIC Family all in one NDIS Driver
;;
;; Copyright 2005, Realtek Semiconductor Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT = netrtle.cat                        ;;for WHQL certified
DriverVer      = 09/20/2007,5.676.0920.2007

[Manufacturer]
%Realtek%   = Realtek, NTx86.5.1, NTamd64

[ControlFlags]
ExcludeFromSelect = PCI\VEN_10EC&DEV_8168
ExcludeFromSelect = PCI\VEN_10EC&DEV_8136

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
;8168C
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02

[Realtek.NTx86.5.1]; This section will only be installed by Windows XP
%RTL8136.DeviceDesc%	= RTL8136x.ndi,	    PCI\VEN_10EC&DEV_8136
%RTL8168.DeviceDesc%	= RTL8168x.ndi,	    PCI\VEN_10EC&DEV_8168
%RTL8136.DeviceDesc%	= RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043
;8168C
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02

[Realtek.NTamd64]; This section will only be installed by Windows XP 64-bit
%RTL8136.DeviceDesc%	= RTL8136a.ndi,	    PCI\VEN_10EC&DEV_8136
%RTL8168.DeviceDesc%  	= RTL8168a.ndi,	    PCI\VEN_10EC&DEV_8168
%RTL8136.DeviceDesc%	= RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC
%RTL8168.DeviceDesc%	= RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043
;8168C
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
[rtl8168.ndi]
DriverVer       = 09/20/2007,676
AddReg          = rtl8168.id.reg, RTLnic.all.reg, RTL8168.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8168C.ndi]
DriverVer       = 09/20/2007,676
AddReg          = rtl8168.id.reg, RTLnic.all.reg, RTL8168C.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8136.ndi]
DriverVer       = 09/20/2007,676
AddReg          = rtl8136.id.reg, RTLnic.all.reg, RTL8136.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
[RTL8168.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, RTLnic.all.reg, RTL8168.common.reg, RTL8168.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8168.ndi.NT.Services]
AddService = RTLE8023, 2, rtsnt.Service, common.EventLog

[RTL8168C.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, RTLnic.all.reg, RTL8168C.common.reg, RTL8168.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8168C.ndi.NT.Services]
AddService = RTLE8023, 2, rtsnt.Service, common.EventLog

[RTL8136.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, RTLnic.all.reg, RTL8136.common.reg, RTL8136.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8136.ndi.NT.Services]
AddService = RTLE8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtenic.sys,,,2

[Rtlnic.CopyFiles9x]
Rtenic.sys,,,2

;;****************************************************************************
;; Windows XP
;;****************************************************************************
[RTL8168x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, RTLnic.all.reg, RTL8168.common.reg, RTL8168.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8168x.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8168Cx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, RTLnic.all.reg, RTL8168C.common.reg, RTL8168.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8168Cx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8136x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, RTLnic.all.reg, RTL8136.common.reg, RTL8136.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8136x.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtenicxp.sys,,,2

;;****************************************************************************
;; Windows XP 64-bit
;;****************************************************************************
[RTL8168a.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, RTLnic.all.reg, RTL8168.common.reg, RTL8168.W2K.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8168a.ndi.NT.Services]
AddService = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

[RTL8168Ca.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, RTLnic.all.reg, RTL8168C.common.reg, RTL8168.W2K.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8168Ca.ndi.NT.Services]
AddService = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

[RTL8136a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, RTLnic.all.reg, RTL8136.common.reg, RTL8136.W2K.reg
CopyFiles       = Rtlnic.CopyFilesX64

[RTL8136a.ndi.NT.Services]
AddService = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

[Rtlnic.CopyFilesX64]
Rtenic64.sys,,,2

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8168.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8168"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

[rtl8136.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8136"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; common parameters
;;****************************************************************************
[RTLnic.all.reg]
HKR,Ndi\params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	type,		0, "edit"
HKR,Ndi\params\NetworkAddress,	default,	0, "000000000000"
HKR,Ndi\params\NetworkAddress,	LimitText,	0, "12"
HKR,Ndi\params\NetworkAddress,	UpperCase,	0, "1"
HKR,Ndi\params\NetworkAddress,	Optional,	0, "1"

[PreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[CpPreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\RTPME
HKR,,RTPME
HKR,Ndi\Params\RxBufLen
HKR,,RxBufLen
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan
HKR,,SuperSwitch

[TsPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan

[RTL8168.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

;HKR,,SuperSwitch,0,"0"

HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5Wake-On-Lan%
HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, "Disable"
HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, "Enable"

;HKR,Ndi\params\AutoSpeedDown,         ParamDesc,  0, %AutoSpeedDown%
;HKR,Ndi\params\AutoSpeedDown,         default,    0, "1"
;HKR,Ndi\params\AutoSpeedDown,         type,       0, "enum"
;HKR,Ndi\params\AutoSpeedDown\enum,    "1",        0, "Enable"
;HKR,Ndi\params\AutoSpeedDown\enum,    "0",        0, "Disable"

[RTL8168C.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "7",        0, "8KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "8",        0, "9KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

;HKR,,SuperSwitch,0,"0"

HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5Wake-On-Lan%
HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, "Disable"
HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, "Enable"

;HKR,Ndi\params\AutoSpeedDown,         ParamDesc,  0, %AutoSpeedDown%
;HKR,Ndi\params\AutoSpeedDown,         default,    0, "1"
;HKR,Ndi\params\AutoSpeedDown,         type,       0, "enum"
;HKR,Ndi\params\AutoSpeedDown\enum,    "1",        0, "Enable"
;HKR,Ndi\params\AutoSpeedDown\enum,    "0",        0, "Disable"

[RTL8136.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

;HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
;HKR,Ndi\params\Jumboframe,        default,    0, "0"
;HKR,Ndi\params\Jumboframe,        type,       0, "enum"
;HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
;HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
;HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5Wake-On-Lan%
HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, "Disable"
HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, "Enable"

[RTL8168.W2K.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

[RTL8136.W2K.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

HKR,,CksOffload,0,"1" 
HKR,,Largesend,0,"1" 

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTLE8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic.sys
LoadOrderGroup  = NDIS

[RTLE8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenicxp.sys
LoadOrderGroup  = NDIS

[RTLE8023x64.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023x64"

[rtsntx64.Service]
DisplayName     = %Rtlnicx64.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFilesX64        = 12
Rtlnic.CopyFiles9x         = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtenic.sys	= 1
Rtenicxp.sys	= 1
Rtenic64.sys	= 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN Tagging"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Offload Checksum"
LargesendOffload	= "Offload TCP_LargeSend"
SpeedDuplexMode		= "Link Speed/Duplex Mode"
auto_nego		= "Auto Negotiation"
sd10half		= "10Mbps/Half Duplex"
sd10full		= "10Mbps/Full Duplex"
sd100half		= "100Mbps/Half Duplex"
sd100full		= "100Mbps/Full Duplex"
sd1000full		= "1000Mbps/Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Number of Tx Descriptor"
;RxDescNumber		= "Number of Rx Descriptor"
;TxHPQDescNumber	= "Number of High Priority Tx Descriptor"
;WOLCapability		= "WakeUp on ARP/PING"
;WOLLinkChange		= "WakeUp on Link Change"
LDPSCapability		= "Link Down Power Saving"
;OptimalPerf		= "Optimal Performance"
FlowControl		= "Flow Control"
AutoSpeedDown		= "Auto Speed Down"
S5Wake-On-Lan		= "Wake-On-Lan After Shutdown"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek RTL8168/8111 PCI-E Gigabit Ethernet NIC"
RTL8168C.DeviceDesc       = "Realtek RTL8168C(P)/8111C(P) PCI-E Gigabit Ethernet NIC"
RTL8136.DeviceDesc        = "Realtek RTL8139/810x Family Fast Ethernet NIC"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"
