;*******************************************************************************
;*                                                                            **
;*                     I N T E L   P R O P R I E T A R Y                      **
;*                                                                            **
;*   COPYRIGHT (c) 1993-2001 BY INTEL CORPORATION. ALL RIGHTS RESERVED.  NO   **
;*   PART  OF  THIS  PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED,   **
;*   TRANSCRIBED, STORED IN A RETRIEVAL  SYSTEM,  OR  TRANSLATED  INTO  ANY   **
;*   LANGUAGE OR COMPUTER LANGUAGE IN ANY FORM OR BY ANY MEANS, ELECTRONIC,   **
;*   MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL, MANUAL, OR OTHERWISE, WITHOUT   **
;*   THE PRIOR WRITTEN PERMISSION OF :                                        **
;*                                                                            **
;*                             INTEL CORPORATION                              **
;*                                                                            **
;*                          2200 MISSION COLLEGE BLVD                         **
;*                                                                            **
;*                     SANTA CLARA, CALIFORNIA 95052-8119                     **
;*                                                                            **
;*******************************************************************************
;
;*******************************************************************************
; NET5579x.INF
; $Revision: 9 $
;
; Intel 82557-based PCI Ethernet Adapters
; PnP install script for Windows 9x
; version 6.1.3

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %V_INTEL%
CatalogFile     = e100bc.cat
DriverVer       = 02/25/2002,6.1.3.0

[Manufacturer]
%V_INTEL%   = Intel

[ControlFlags]
ExcludeFromSelect =  \
                        PCI\VEN_8086&DEV_1229&SUBSYS_00018086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00028086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00038086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_000B8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_000C8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00308086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00418086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_05,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10308086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10418086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10518086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10528086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_04,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_05,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21038086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22018086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24028086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24098086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_240F8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24108086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24128086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_005C1014&REV_04,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_005C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_105C1014&REV_08,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_105C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01F11014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01F21014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_02071014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_023F1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_305C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_405C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_505C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_605C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_705C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_805C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10C0103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10C3103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10CA103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10CB103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10E3103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10E4103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_1200103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30010E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30020E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30030E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30040E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30050E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30060E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30070E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_009B1028&REV_08,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00708086,\
                        PCI\VEN_8086&DEV_1229&REV_01,\
                        PCI\VEN_8086&DEV_1229&REV_02,\
                        PCI\VEN_8086&DEV_1229&REV_04,\
                        PCI\VEN_8086&DEV_1229&REV_05,\
                        PCI\VEN_8086&DEV_1229&REV_08,\
                        PCI\VEN_8086&DEV_1229&REV_09,\
                        PCI\VEN_8086&DEV_1229&REV_0C,\
                        PCI\VEN_8086&DEV_1229&REV_0D,\
                        PCI\VEN_8086&DEV_1229&REV_0E,\
                        PCI\VEN_8086&DEV_1229&REV_0F,\
                        PCI\VEN_8086&DEV_1229&REV_10,\
                        PCI\VEN_8086&DEV_1059


[Intel]
; DisplayName                Section        DeviceID
; -----------                -------        --------
%PCIE10PPCI.DeviceDesc%  =E10P.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00038086

%PCIE100BTX.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00018086
%PCIE100BT4.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00028086
%PCIE100RWU.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00048086
%I557IFE.DeviceDesc%            = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00058086
%I557IFEWFM.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00068086

%I558IFE.DeviceDesc%            = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_00078086
%I558IFEWFM.DeviceDesc%         = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_00088086
%PCIE100PLUS.DeviceDesc%        = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00098086
%PCIE100MAN.DeviceDesc%         = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000A8086

%PCIE100PLUS.DeviceDesc%        = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000B8086
%PCIE100MAN.DeviceDesc%         = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000C8086
%PCIE100AOL.DeviceDesc%         = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000D8086
%PCIE100MANAOL.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000E8086
%PCIE100S0.DeviceDesc%          = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000F8086

%PCIE100S.DeviceDesc%           = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00108086
%PCIE100S.DeviceDesc%           = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00118086
%PCIE100SADV.DeviceDesc%        = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00128086
%PCIE100SADV.DeviceDesc%        = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00138086

%PCIE100MANAOLGC.DeviceDesc%    = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00308086
%PCIE100S0.DeviceDesc%          = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00318086
%PCIE100Sx.DeviceDesc%          = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00408086
%PCIE100Sx.DeviceDesc%          = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00418086
%PCIE100S0.DeviceDesc%          = D102SCN.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00428086

%PCIE100Sx.DeviceDesc%          = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00508086
%PCIE100Sx.DeviceDesc%          = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00518086
%PCIE100DUALx.DeviceDesc%       = D102m0.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10148086
%PCIE100DUALSx.DeviceDesc%      = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10158086
%PCIE100DUALSx.DeviceDesc%      = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10168086
%PCIE100SxSVR.DeviceDesc%       = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10508086

%PCIE100BSPLUSD.DeviceDesc%     = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00608086
%PCIE100BSPLUSS.DeviceDesc%     = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10608086

%PCIE100SCBLAN.DeviceDesc%      = D102mCB.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_20168086
%PCIE100SCBCOMBO.DeviceDesc%    = D102mCB.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_20178086
%PCIE100SCBLANR.DeviceDesc%     = D102mCB.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_20188086
%PCIE100SCBCOMBOR.DeviceDesc%   = D102mCB.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_20198086

%PCIE100SxL.DeviceDesc%         = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30108086
%PCIE100SxL.DeviceDesc%         = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30118086
%PCIE100S0L.DeviceDesc%         = D102m0.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30128086

%PCIE100B.DeviceDesc%           = D102mCm.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00011179 ; 82550 rev D
%IBMFEE.DeviceDesc%             = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_02321014

%PCIE100SERVER.DeviceDesc%      = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_04
%PCIE100SERVER.DeviceDesc%      = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_05
%PCIE100SERVERW.DeviceDesc%     = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_100C8086
%PCIE100SSVR.DeviceDesc%        = D101SS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10128086
%PCIE100SSVR.DeviceDesc%        = D101SS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10138086
%PCIE100DUAL.DeviceDesc%        = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10178086
%PCIE100MANAOLGS.DeviceDesc%    = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10308086
%PCIE100SxSVR.DeviceDesc%       = D102SSC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10408086
%PCIE100SxSVR.DeviceDesc%       = D102SSC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10418086
%PCIE100S0SVR.DeviceDesc%       = D102SSCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10428086
%PCIE100S0SVR.DeviceDesc%       = D102SSCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10518086
%PCIE100S0SVR.DeviceDesc%       = D102SSCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10528086
%PCIE100DUAL.DeviceDesc%        = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_04
%PCIE100DUAL.DeviceDesc%        = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_05

%PCIE100SCBLAN.DeviceDesc%      = D102MCBS.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20098086
%PCIE100CBLAN.DeviceDesc%       = D101MCB.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_200D8086
%PCIE100CBCOMBO.DeviceDesc%     = D101MCBC.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_200E8086
%PCIE100SCBLANR.DeviceDesc%     = D102MCBS.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_200F8086
%PCIE100SCBCOMBO.DeviceDesc%    = D102MCBS.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20108086
%PCIE100SCBCOMBOR.DeviceDesc%   = D102MCBS.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20138086

%PCIE100SCBLANNODES.DeviceDesc% = D102MCBSNODES.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20118086
%PCIE100SCBCOMBONODES.DeviceDesc% = D102MCBSNODES.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20128086
%PCIE100SCBRCOMBONODES.DeviceDesc% = D102MCBSNODES.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20148086
%PCIE100SCBLANRNODES.DeviceDesc% = D102MCBSNODES.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_20158086

%MiniPCI3A.DeviceDesc%          = D102MP.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_21008086
%MiniPCI.DeviceDesc%            = D102MP.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_21018086
%MiniPCIDes.DeviceDesc%         = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_21028086
%MiniPCIDes.DeviceDesc%         = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_21038086
%MiniPCIDes.DeviceDesc%         = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_21048086
%MiniPCIDes.DeviceDesc%         = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_21058086
%MiniPCI.DeviceDesc%            = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_21068086
%MiniPCILON.DeviceDesc%         = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_21078086
%MiniPCILON.DeviceDesc%         = D102MP.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_21088086

%MiniPCICombo.DeviceDesc%       = D102MP.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_22008086
%MiniPCICombo.DeviceDesc%       = D102MP.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_22018086
%MiniPCIComboDes.DeviceDesc%    = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_22028086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_22038086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_22048086
%MiniPCIComboDes.DeviceDesc%    = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_22058086
%MiniPCIComboDes.DeviceDesc%    = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_22068086
%MiniPCIComboDes.DeviceDesc%    = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_22078086
%MiniPCICombo.DeviceDesc%       = D102MP.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_22088086

%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24028086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24078086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24088086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24098086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_240F8086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24108086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24118086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24128086
%I559CMiniPCI.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_24138086

%I559IFE.DeviceDesc%            = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30008086
%I559IFEAOL.DeviceDesc%         = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30018086
%I559IFEAOLII.DeviceDesc%       = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30028086
%PCIE100SxL.DeviceDesc%         = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30068086
%PCIE100SxL.DeviceDesc%         = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30078086
%PCIE100S0L.DeviceDesc%         = D102SCN.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_30088086
%PCIE100LAVON.DeviceDesc%       = Lavon.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00708086

; IBM with intel device name

%I559CLONPCI.DeviceDesc%        = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_B2090E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30010E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30020E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30030E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30040E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30050E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30060E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30070E11

%HPTX.DeviceDesc%               = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10C0103C
%HPTX.DeviceDesc%               = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10C3103C
%HPTX.DeviceDesc%               = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10CA103C
%HPTX.DeviceDesc%               = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10CB103C
%HPTX.DeviceDesc%               = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10E3103C
%HPTX.DeviceDesc%               = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10E4103C
%HPTX.DeviceDesc%               = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_1200103C

%IBMFE2.DeviceDesc%             = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_005C1014&REV_05
%IBMFE2.DeviceDesc%             = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_005C1014&REV_04
%IBMFE1.DeviceDesc%             = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_005C1014
%IBMFE9.DeviceDesc%             = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014
%IBMFEC.DeviceDesc%             = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01F11014
%IBMFEC.DeviceDesc%             = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01F21014
%IBMFED.DeviceDesc%             = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_02071014
%IBMFED.DeviceDesc%             = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_023F1014
%IBMFE2.DeviceDesc%             = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_105C1014&REV_08
%IBMFE2.DeviceDesc%             = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_105C1014
%IBMFE3.DeviceDesc%             = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_305C1014
%IBMFE4.DeviceDesc%             = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_405C1014
%IBMFE5.DeviceDesc%             = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_505C1014
%IBMFE6.DeviceDesc%             = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_605C1014
%IBMFE7.DeviceDesc%             = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_705C1014
%IBMFE8.DeviceDesc%             = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_805C1014

%SamsungMiniPCI.DeviceDesc%     = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_2501144D
%SamsungILMiniPCI.DeviceDesc%   = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_2502144D

%Toshiba82559B.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00031179

%9821XB06.DeviceDesc%            = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_80001033
%PKUGX06.DeviceDesc%             = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_80161033
%PKUGX06.DeviceDesc%             = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_801F1033
%PKUGX06.DeviceDesc%             = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_80261033
%NEC82559BASED.DeviceDesc%       = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_80631033
%NEC82559BASED.DeviceDesc%       = D101SMP.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_80641033
%NEC82559BASED.DeviceDesc%       = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_80C41033

%PCIE100B.DeviceDesc%            = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_111510CF
%PCIE100B.DeviceDesc%            = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_114310CF

; Fujitsu
%PCIE100B.DeviceDesc%            = D102MPS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_111510CF
%PCIE100B.DeviceDesc%            = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_114310CF

;Siemens
%Siemens558Wol.DeviceDesc%      = D101r5.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_0019110A
%SiemensLan.DeviceDesc%         = D101r5.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_0031110A
%Siemens559Wol.DeviceDesc%      = D101M.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_0037110A
%SiemensWolAol.DeviceDesc%      = D101SG.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_004B110A
%Siemens558.DeviceDesc%         = D101r5.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_6608110A
%Siemens559C.DeviceDesc%        = D101M.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_6618110A

;Dell Viper
%PCIE100B.DeviceDesc%           = D101MG.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_009B1028&REV_08

;Intel Generic catchalls
%PCIE100B.DeviceDesc%           = E100B.ndi,    PCI\VEN_8086&DEV_1229&REV_01
%PCIE100B.DeviceDesc%           = E100B.ndi,    PCI\VEN_8086&DEV_1229&REV_02
%PCIE100B.DeviceDesc%           = D101.ndi,     PCI\VEN_8086&DEV_1229&REV_04
%PCIE100B.DeviceDesc%           = D101r5.ndi,   PCI\VEN_8086&DEV_1229&REV_05
%PCIE100B.DeviceDesc%           = D101MG.ndi,   PCI\VEN_8086&DEV_1229&REV_08
%PCIE100B.DeviceDesc%           = D101SG.ndi,   PCI\VEN_8086&DEV_1229&REV_09
%PCIE100B.DeviceDesc%           = D102SCNG.ndi, PCI\VEN_8086&DEV_1229&REV_0C
%PCIE100B.DeviceDesc%           = D102mG.ndi,   PCI\VEN_8086&DEV_1229&REV_0D
%PCIE100B.DeviceDesc%           = D102mG.ndi,   PCI\VEN_8086&DEV_1229&REV_0E
%PCIE100LAVONLOM.DeviceDesc%    = Lavon.ndi,    PCI\VEN_8086&DEV_1229&REV_0F
%PCIE100LAVONLOM.DeviceDesc%    = Lavon.ndi,    PCI\VEN_8086&DEV_1229&REV_10
%PCIE100LAVONMB.DeviceDesc%     = Lavonmb.ndi,  PCI\VEN_8086&DEV_1059&REV_0F
%PCIE100LAVONMB.DeviceDesc%     = Lavonmb.ndi,  PCI\VEN_8086&DEV_1059&REV_10

;--- 82557 Rev 1, 2
;
[E100B.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82558 Rev 4
;
[D101.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82558 Rev 5
;
[D101r5.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, PowerSave.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 8
;
[D101M.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 8 Generic
;
[D101MG.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Cardbus Adapter D101M Rev 8
;
[D101MCB.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, CPUSaverOverride.reg, EnablePME.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Cardbus Combo D101M Rev 8
;
[D101MCBC.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, CPUSaverOverride.reg, EnablePME.reg, e100b.ndi.reg, Clkrun.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 9 Security
;
[D101S.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 9 Security Generic
;
[D101SG.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.reg, Security.reg, SecOff.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- D101S Rev 9 Server
;
[D101SS.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 MiniPCI
;
[D101SMP.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, e100b.ndi.reg, SecDisable.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Security Cardbus
;
[D102MCBS.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, CPUSaverOverride.reg, EnablePME.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Cardbus No DES
;
[D102MCBSNODES.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, CPUSaverOverride.reg, EnablePME.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Server
;
[D102SC.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C
;
[D102SCN.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, SecDisable.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Generic
;
[D102SCNG.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.reg, Security.reg, SecOff.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Security Server
;
[D102SSC.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Server
;
[D102SSCN.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, SecDisable.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C MiniPCI
;
[D102MP.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, e100b.ndi.reg, SecDisable.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles


;--- 82550 Rev C MiniPCI Security
;
[D102MPS.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Server
;
[D102mS.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Client
;
[D102mC.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Client Mobile
;
[D102mCm.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, EnableLLPD.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Server NoDes
;
[D102m0.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Security Cardbus
;
[D102mCB.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, CPUSaverOverride.reg, EnablePME.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev F Lavon mobile
;
[Lavonmb.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, EnablePME.reg, e100b.ndi.reg, LogLinkState.reg, DisableLinkInterrupt.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Generic
;
[D102mG.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, EnablePME.reg, e100b.ndi.reg, Security.reg, SecOff.reg, LLPDD_OFF.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev F Lavon
;
[Lavon.ndi]
DriverVer       = 02/25/2002,6.1.3.0
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Intel(R) PRO/10+ PCI Adapter
;
[E10P.ndi]
DriverVer       = 02/25/2002,6.1.3.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed10.reg, 82557.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Common 82557 NDI parameters
;
[82557.reg]
HKR,Ndi\Params\NumRfd,                ParamDesc,  0, "Receive Buffers"
HKR,Ndi\Params\NumRfd,                Type,       0, "int"
HKR,Ndi\Params\NumRfd,                Default,    0, "48"
HKR,Ndi\Params\NumRfd,                Min,        0, "8"
HKR,Ndi\Params\NumRfd,                Max,        0, "1024"
HKR,Ndi\Params\NumRfd,                Step,       0, "1"
HKR,Ndi\Params\NumRfd,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumRfd,   MiniHelp,   0, "Number of buffers used by the driver when copying data to the protocol memory."

HKR,Ndi\Params\NumTcb,                ParamDesc,  0, "Transmit Control Blocks"
HKR,Ndi\Params\NumTcb,                Type,       0, "int"
HKR,Ndi\Params\NumTcb,                Default,    0, "16"
HKR,Ndi\Params\NumTcb,                Min,        0, "8"
HKR,Ndi\Params\NumTcb,                Max,        0, "64"
HKR,Ndi\Params\NumTcb,                Step,       0, "1"
HKR,Ndi\Params\NumTcb,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumTcb,   MiniHelp,   0, "Sets the number of control blocks available for adapter use."

HKR,Ndi\Params\NumCoalesce,           ParamDesc,  0, "Coalesce Buffers"
HKR,Ndi\Params\NumCoalesce,           Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,           Default,    0, "8"
HKR,Ndi\Params\NumCoalesce,           Min,        0, "1"
HKR,Ndi\Params\NumCoalesce,           Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,           Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,           Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumCoalesce, MiniHelp, 0, "Number of buffers available for transmits acceleration."

HKR,Ndi\Params\Adaptive_IFS,          ParamDesc,  0, "Adaptive Inter-Frame Spacing"
HKR,Ndi\Params\Adaptive_IFS,          Type,       0, "int"
HKR,Ndi\Params\Adaptive_IFS,          Default,    0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Min,        0, "0"
HKR,Ndi\Params\Adaptive_IFS,          Max,        0, "255"
HKR,Ndi\Params\Adaptive_IFS,          Step,       0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Adaptive_IFS, MiniHelp, 0, "Compensates for excessive Ethernet packet collisions."

HKR,Ndi\Params\Threshold,             ParamDesc,  0, "Adaptive Transmit Threshold"
HKR,Ndi\Params\Threshold,             Type,       0, "int"
HKR,Ndi\Params\Threshold,             Default,    0, "12"
HKR,Ndi\Params\Threshold,             Min,        0, "0"
HKR,Ndi\Params\Threshold,             Max,        0, "200"
HKR,Ndi\Params\Threshold,             Step,       0, "1"
HKR,Ndi\Params\Threshold,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Threshold, MiniHelp,  0, "Sets number of bytes before adapter empties its FIFO buffer. Actual value is 8 times setting."

HKR,Ndi\Params\HPQPriorityLevel,             ParamDesc,  0, "Priority Level Definition"
HKR,Ndi\Params\HPQPriorityLevel,             Type,       0, "int"
HKR,Ndi\Params\HPQPriorityLevel,             Default,    0, "4"
HKR,Ndi\Params\HPQPriorityLevel,             Min,        0, "0"
HKR,Ndi\Params\HPQPriorityLevel,             Max,        0, "7"
HKR,Ndi\Params\HPQPriorityLevel,             Step,       0, "1"
HKR,Ndi\Params\HPQPriorityLevel,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\HPQPriorityLevel, MiniHelp,  0, "Sets the controlled cutoff level for using HPQ."

HKR,Ndi\Params\UcodeSW,               ParamDesc,  0, "Adaptive Technology"
HKR,Ndi\Params\UcodeSW,               Type,       0, "enum"
HKR,Ndi\Params\UcodeSW,               Default,    0, "1"
HKR,Ndi\Params\UcodeSW\Enum,          "1",        0, "On"
HKR,Ndi\Params\UcodeSW\Enum,          "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\UcodeSW,  MiniHelp,   0, "Enables/Disables the Adaptive Technology performance feature."

HKR,Ndi\Params\Coalesce,              ParamDesc,  0, "PCI Bus Efficiency"
HKR,Ndi\Params\Coalesce,              Type,       0, "enum"
HKR,Ndi\Params\Coalesce,              Default,    0, "0"
HKR,Ndi\Params\Coalesce\Enum,         "1",        0, "Enabled"
HKR,Ndi\Params\Coalesce\Enum,         "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\Coalesce, MiniHelp,   0, "Coalesces transmit packets into single buffer before sending them to network."

HKR,Ndi\Params\AlwaysConnectGoal,              ParamDesc,  0, "Basic Connectivity For No Resources"
HKR,Ndi\Params\AlwaysConnectGoal,              Type,       0, "enum"
HKR,Ndi\Params\AlwaysConnectGoal,              Default,    0, "1"
HKR,Ndi\Params\AlwaysConnectGoal\Enum,         "1",        0, "Enabled"
HKR,Ndi\Params\AlwaysConnectGoal\Enum,         "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\AlwaysConnectGoal, MiniHelp,   0,  "Try to load the driver in low resources environment."

HKR,PROSetNdi\Params\NetworkAddress,  ParamDesc,  0, "Locally Administered Address"
HKR,PROSetNdi\Params\NetworkAddress,  Type,       0, "edit"
HKR,PROSetNdi\Params\NetworkAddress,  Default,    0, ""
HKR,PROSetNdi\Params\NetworkAddress,  Base,       0, "16"
HKR,PROSetNdi\Params\NetworkAddress,  MiniHelp,   0, "Allows you to change the network address."

HKR,Ndi\Params\ConfigIFS,                ParamDesc,  0, "Retransmit Inter-Frame Spacing"
HKR,Ndi\Params\ConfigIFS,                Type,       0, "int"
HKR,Ndi\Params\ConfigIFS,                Default,    0, "6"
HKR,Ndi\Params\ConfigIFS,                Min,        0, "0"
HKR,Ndi\Params\ConfigIFS,                Max,        0, "15"
HKR,Ndi\Params\ConfigIFS,                Step,       0, "1"
HKR,Ndi\Params\ConfigIFS,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\ConfigIFS,   MiniHelp,   0, "Compensates for excessive Ethernet packet collisions by controlling retransmit timing."

HKR,,PcNic,                     0, "1"
HKR,,MWIEnable,                 2, "0"
HKR,,AdaptiveStalledInterrupts, 2, "1"
HKR,,AdaptiveCarrierLoss,       2, "1"
HKR,,AdaptiveTransmitMethod,    2, "1"

HKR,,DeviceVxDsPrefix,          0, "e100b"

;--- 82558 ACPI Wake On LAN parameter
;
[AcpiWol.reg]
HKR,Ndi\Params\AcpiWol,               ParamDesc,  0, "ACPI Wake On LAN"
HKR,Ndi\Params\AcpiWol,               Type,       0, "enum"
HKR,Ndi\Params\AcpiWol,               Default,    0, "1"
HKR,Ndi\Params\AcpiWol\Enum,          "1",        0, "Enabled"
HKR,Ndi\Params\AcpiWol\Enum,          "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\AcpiWol,  MiniHelp,   0, "Enables or disables the Magic Packet* service for Wake On LAN with Windows 98 version 4.10.1998."

HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,Start,     1, 00
HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,StaticVxD, 0, "WOL558.vxd"

;--- Log Link State Event
;
[LogLinkState.reg]
HKR,,LogLinkStateEvent, 0,      "1"

;--- 82558 specifics
;
[82558.reg]
; 802.1p/802.1q Packet Tagging
HKR,Ndi\Params\TaggingMode,         ParamDesc,  0, "QoS Packet Tagging"
HKR,Ndi\Params\TaggingMode,         Type,       0, "enum"
HKR,Ndi\Params\TaggingMode,         Default,    0, "0"
HKR,Ndi\Params\TaggingMode\Enum,    "1",        0, "Enabled"
HKR,Ndi\Params\TaggingMode\Enum,    "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\TaggingMode, MiniHelp, 0, "Send and receive IEEE Tagged frames (802.3ac/802.1p/802.1Q)."

HKR,Ndi\Params\FlowControl,              ParamDesc,  0, "Flow Control Settings"
HKR,Ndi\Params\FlowControl,              Type,       0, "enum"
HKR,Ndi\Params\FlowControl,              Default,    0, "0"
HKR,Ndi\Params\FlowControl\Enum,         "3",        0, "Generate and Respond"
HKR,Ndi\Params\FlowControl\Enum,         "2",        0, "Respond"
HKR,Ndi\Params\FlowControl\Enum,         "1",        0, "Generate"
HKR,Ndi\Params\FlowControl\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\FlowControl, MiniHelp,   0, "Pauses packet transmission on receipt of full flow control frame and Send full flow control frame to notify the other side to stop transmission."

; Adaptive Performance Tuning
HKR,PROSetNdi\Params\CPUSaver,        ParamDesc,  0, "Adaptive Performance Tuning"
HKR,PROSetNdi\Params\CPUSaver,        Type,       0, "slider"
HKR,PROSetNdi\Params\CPUSaver,        Default,    0, "512"
HKR,,CPUSaver,                                    0, "512"
HKR,PROSetNdi\Params\CPUSaver,        LeftLabel,  0, "Adapter Bandwidth"
HKR,PROSetNdi\Params\CPUSaver,        RightLabel, 0, "CPU Utilization"
HKR,PROSetNdi\Params\CPUSaver,        MiniHelp,   0, "Sets optimal point of CPU/Adapter performance for this system."
HKR,PROSetNdi\Params\CPUSaver\Values, "0",        0, "0"
HKR,PROSetNdi\Params\CPUSaver\Values, "1",        0, "1"
HKR,PROSetNdi\Params\CPUSaver\Values, "2",        0, "512"
HKR,PROSetNdi\Params\CPUSaver\Values, "3",        0, "768"
HKR,PROSetNdi\Params\CPUSaver\Values, "4",        0, "1024"
HKR,PROSetNdi\Params\CPUSaver\Values, "5",        0, "1280"
HKR,PROSetNdi\Params\CPUSaver\Values, "6",        0, "1536"
HKR,PROSetNdi\Params\CPUSaver\Values, "7",        0, "1792"
HKR,PROSetNdi\Params\CPUSaver\Values, "8",        0, "2048"
HKR,PROSetNdi\Params\CPUSaver\Values, "9",        0, "2304"
HKR,PROSetNdi\Params\CPUSaver\Values, "10",       0, "2560"
HKR,PROSetNdi\Params\CPUSaver\Values, "11",       0, "2816"
HKR,PROSetNdi\Params\CPUSaver\Values, "12",       0, "3072"
HKR,PROSetNdi\Params\CPUSaver\Values, "13",       0, "3328"
HKR,PROSetNdi\Params\CPUSaver\Values, "14",       0, "3584"
HKR,PROSetNdi\Params\CPUSaver\Values, "15",       0, "3840"
HKR,PROSetNdi\Params\CPUSaver\Values, "16",       0, "4096"

;--- 82558 B Rev 5
;--- 82558 B Rev 5 - no force wake on link
;
[82558B.reg]
; WakeOn
HKR, PROSetNdi\Params\WakeOn,       ParamDesc,          0, "Wake on Settings"
HKR, PROSetNdi\Params\WakeOn,       default,            0, "1014"
HKR, PROSetNdi\Params\WakeOn\Enum,  "1",                0, "Wake on Link Change"
HKR, PROSetNdi\Params\WakeOn\Enum,  "2",                0, "Wake on Magic Packet"
HKR, PROSetNdi\Params\WakeOn\Enum,  "4",                0, "Wake on LAA"
HKR, PROSetNdi\Params\WakeOn\Enum,  "48",               0, "Wake on ARP"
HKR, PROSetNdi\Params\WakeOn\Enum,  "80",               0, "Wake on directed packet"
HKR, PROSetNdi\Params\WakeOn\Enum,  "144",              0, "Wake on NBT Query"
HKR, PROSetNdi\Params\WakeOn,       type,               0, "bitfield"
HKR, PROSetNdi\Params\WakeOn,       ExposeLevel,        0, "2"
HKR,,                                                      WakeOn,  2, "1014"
HKR,PROSetNdi\Params\WakeOn,        MiniHelp,   0,      "Determines how to Wake up the system (Link Change, Magic Packet, Pattern Matching, etc.)."


;--- 82558 B Rev 5 - with force wake on link enabled
;
[82558B_forcewakeonlink.reg]
; WakeOn
HKR, PROSetNdi\Params\WakeOn,       ParamDesc,          0, "Wake on Settings"
HKR, PROSetNdi\Params\WakeOn,       default,            0, "1014"
HKR, PROSetNdi\Params\WakeOn\Enum,  "1",                0, "Wake on Link Change"
HKR, PROSetNdi\Params\WakeOn\Enum,  "2",                0, "Wake on Magic Packet"
HKR, PROSetNdi\Params\WakeOn\Enum,  "4",                0, "Wake on LAA"
HKR, PROSetNdi\Params\WakeOn\Enum,  "48",               0, "Wake on ARP"
HKR, PROSetNdi\Params\WakeOn\Enum,  "80",               0, "Wake on directed packet"
HKR, PROSetNdi\Params\WakeOn\Enum,  "144",              0, "Wake on NBT Query"
HKR, PROSetNdi\Params\WakeOn,       type,               0, "bitfield"
HKR, PROSetNdi\Params\WakeOn,       ExposeLevel,        0, "2"
HKR,,                                                      WakeOn,  2, "1014"
HKR,PROSetNdi\Params\WakeOn,        MiniHelp,   0,      "Determines how to Wake up the system (Link Change, Magic Packet, Pattern Matching, etc.)."

HKR,Ndi\Params\ForceWakeOnLink,             ParamDesc,  0, "Force Wake On Link"
HKR,Ndi\Params\ForceWakeOnLink,             Type,       0, "enum"
HKR,Ndi\Params\ForceWakeOnLink,             Default,    0, "0"
HKR,Ndi\Params\ForceWakeOnLink\Enum,        "1",        0, "Enabled"
HKR,Ndi\Params\ForceWakeOnLink\Enum,        "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\ForceWakeOnLink, MiniHelp,  0, "When enabled, forces system to wake on link change"


;--- 82559 Enable PME
;
[EnablePME.reg]
HKR,Ndi\Params\EnablePME,             ParamDesc,  0, "Enable PME"
HKR,Ndi\Params\EnablePME,             Type,       0, "enum"
HKR,Ndi\Params\EnablePME,             Default,    0, "2"
HKR,Ndi\Params\EnablePME\Enum,        "1",        0, "Enabled"
HKR,Ndi\Params\EnablePME\Enum,        "0",        0, "Disabled"
HKR,Ndi\Params\EnablePME\Enum,        "2",        0, "No Action"
HKR,Ndi\Params\EnablePME\Enum,        "255",      0, "Hardware Default"
HKR,PROSetNdi\NdiExt\Params\EnablePME, MiniHelp,  0, "Allows wake-up from APM power management when enabled. Disable shuts down LAN controller under ACPI"

;--- Clkrun
[Clkrun.reg]
HKR,,CLKRUN,                                      0, "1"

;--- Enable Power Down
;
[EnableLLPD.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      ParamDesc,  0, "Smart Power Down"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Type,       0, "enum"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "1"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "1",        0, "Enabled"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\EnablePowerDownOnLinkLoss, MiniHelp, 0, "Removes adapter power when LAN cable disconnected."

HKR,Ndi\Params\LinkBasedLogin,              ParamDesc,  0, "Adaptive Link Response"
HKR,Ndi\Params\LinkBasedLogin,              Type,       0, "enum"
HKR,Ndi\Params\LinkBasedLogin,              Default,    0, "0"
HKR,Ndi\Params\LinkBasedLogin\Enum,         "1",        0, "On"
HKR,Ndi\Params\LinkBasedLogin\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\LinkBasedLogin, MiniHelp,   0, "Enables Adaptive Link Response to check PHYLink status."

;--- Expose Power Mangement feature in Lavon
[PowerSave.reg]
HKR,,AutoPowerSaveModeEnabled, 0, "1"
HKR,,Force10MbOnD3, 0, "1"

[LLPDD_OFF.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "0"

[DisableLinkInterrupt.reg]
HKR,,LinkInterruptEnabled,  0, "0"

;--- Security
;
[Security.reg]
HKR,Ndi\Params\MaxNumSecAssoc,  ParamDesc,  0, %SecurityAssociations%
HKR,Ndi\Params\MaxNumSecAssoc,  Type,       0, "int"
HKR,Ndi\Params\MaxNumSecAssoc,  Default,    0, "64"     ; Client
HKR,Ndi\Params\MaxNumSecAssoc,  Min,        0, "1"
HKR,Ndi\Params\MaxNumSecAssoc,  Max,        0, "5000"
HKR,Ndi\Params\MaxNumSecAssoc,  Step,       0, "1"
HKR,Ndi\Params\MaxNumSecAssoc,  Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\MaxNumSecAssoc, MiniHelp, 0, "Simultaneous Security Associations that can be offloaded to the adapters co-processor."

HKR,Ndi\Params\TaskOffload,     ParamDesc,  0, %TaskOffload%
HKR,Ndi\Params\TaskOffload,     Type,       0, "enum"
HKR,Ndi\Params\TaskOffload,     Default,    0, "1"
HKR,Ndi\Params\TaskOffload\Enum,"0",        0, %None%
HKR,Ndi\Params\TaskOffload\Enum,"1",        0, %Ipsecurity%
HKR,PROSetNdi\NdiExt\Params\TaskOffload, MiniHelp, 0, "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."

HKR,,IPSecTunnelMode, 2, "1"
HKR,,MaxNumSecAssoc,  2, "64"

[SecSerDef.reg]
HKR,Ndi\Params\MaxNumSecAssoc,  Default,    0, "1000"   ; Server

[SecOff.reg]
HKR,Ndi\Params\TaskOffload,     Default,    0, "0"

[SecDisable.reg]
HKR,,TaskOffload,    0, "0"

;--- Checksum Offload
;
[CSumOffload.reg]
HKR,Ndi\Params\TaskOffload,     ParamDesc,  0, %TaskOffload%
HKR,Ndi\Params\TaskOffload,     Type,       0, "enum"
HKR,Ndi\Params\TaskOffload,     Default,    0, "2"
HKR,Ndi\Params\TaskOffload\Enum,"0",        0, %None%
HKR,Ndi\Params\TaskOffload\Enum,"2",        0, %Checksum_str%
HKR,PROSetNdi\NdiExt\Params\TaskOffload,  MiniHelp, 0, "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."

;--- CPUSaver override for Cardbus
;
[CPUSaverOverride.reg]
HKR,PROSetNdi\Params\CPUSaver,  Default,    0, "1"
HKR,,CPUSaver,                              0, "1"

;--- Speed Duplex Mode common base 10Mb
;
[Speed10.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "1"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp, 0, "Sets link speed to 10 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."

;--- Speed Duplex Mode common base 10/100Mb
;
[Speed100.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "0"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp, 0, "Sets link speed to 10/100 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."

;--- Settings to be cleaned up
;
[8255x_Legacy.DelReg]
HKR,Ndi\Params\Eid
HKR,Ndi\Params\MapRegisters
HKR,,Eid
HKR,,MapRegisters

;--- Win9x NDI object registration
;
[E100B.ndi.reg]
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "e100bnt5.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,,               Driver,           0, "e100bnt.sys"
HKR,NDIS,           LogDriverName,    0, "E100B"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,NDIS\ODI,       DriverName,       0, "e100bodi"
HKR,NDIS\ODI,       FileName,         0, "e100bodi.com"
HKR,Ndi,            NdiInstaller,     0, "8255indi.dll,i557NdiProc"
HKR,Ndi,            DeviceID,         0, "PCI\VEN_8086&DEV_1229"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3,odi"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"
HKR,Ndi\Install,    odi,              0, "E100B.odi"

;--- Uninstallation
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,DisplayName, 0, "Intel(R) PRO Ethernet Adapter and Software"
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,UninstallString, 0, "8255xDel.exe"

;--- Driver Install
;
; NDIS5
[E100B.ndis5]
CopyFiles = E100B.ndis5.CopyFiles

; NDIS4
[E100B.ndis4]
CopyFiles = E100B.ndis4.CopyFiles

; NDIS3
[E100B.ndis3]
CopyFiles = E100B.ndis3.CopyFiles

; ODI
[E100B.odi]
CopyFiles = E100B.odi.CopyFiles

;--- Copy files
;
[DestinationDirs]
DefaultDestDir            = 11

[SourceDisksNames]
1 = %DISKNAME%,,,

[SourceDisksFiles]
net82557.din = 1
8255indi.dll = 1
wol558.vxd   = 1
e100bnt5.sys = 1
e100bnt.sys  = 1
e100b.sys    = 1
e100bodi.com = 1
8255xDel.exe = 1

; Install NDI Helper Dll
[E100B.ndi.copyfiles]
8255indi.dll,,,2
e100bnt5.sys,,,2
WOL558.vxd,,,2
8255xDel.exe,,,2
net82557.din,,,2

[E100B.ndis5.CopyFiles]
e100bnt5.sys,,,2
WOL558.vxd,,,2

[E100B.ndis4.CopyFiles]
e100bnt.sys,,,2

[E100B.ndis3.CopyFiles]
e100b.sys,,,2

[E100B.odi.CopyFiles]
e100bodi.com,,,2

[SpeedDpx.DelReg]
HKR,Ndi\Params\Speed
HKR,Ndi\Params\ForceDpx
HKR,Ndi\Params\PacketTagging
HKR,,Speed
HKR,,ForceDpx
HKR,,PacketTagging

;--- Localizable Strings
;
[Strings]
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

; Parameters
AutoDetect               = "Auto Detect"
SpeedDuplex              = "Link Speed & Duplex"
10Mb-Half-Duplex         = "10Mbps/Half Duplex"
10Mb-Full-Duplex         = "10Mbps/Full Duplex"
100Mb-Half-Duplex        = "100Mbps/Half Duplex"
100Mb-Full-Duplex        = "100Mbps/Full Duplex"
None                     = "None"
Ipsecurity               = "IP Security"
Checksum_str             = "Checksum"
TaskOffload              = "Offloading"
SecurityAssociations     = "Security Associations"

; Device descriptions
PCIE100B.DeviceDesc       = "Intel 8255x-based PCI Ethernet Adapter (10/100)"
PCIE100BTX.DeviceDesc     = "Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc     = "Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc     = "Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc     = "Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc        = "Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc     = "82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc        = "Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc     = "Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc    = "Intel(R) PRO/100+ PCI Adapter"
PCIE100MAN.DeviceDesc     = "Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc  = "Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc = "Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc    = "Intel(R) PRO/100+ Dual Port Server Adapter"
PCIE100CBLAN.DeviceDesc   = "Intel(R) PRO/100 CardBus II"
PCIE100CBCOMBO.DeviceDesc = "Intel(R) PRO/100 LAN+Modem56 CardBus II"
PCIE100SCBLAN.DeviceDesc  = "Intel(R) PRO/100 S Mobile Adapter"
PCIE100SCBLANR.DeviceDesc = "Intel(R) PRO/100 SR Mobile Adapter"
PCIE100SCBCOMBO.DeviceDesc= "Intel(R) PRO/100 S Mobile Combo Adapter"
PCIE100SCBCOMBOR.DeviceDesc="Intel(R) PRO/100 SR Mobile Combo Adapter"
PCIE100AOL.DeviceDesc     = "Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc  = "Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc= "Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc= "Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559CLONPCI.DeviceDesc    = "Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFE.DeviceDesc        = "Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc     = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc   = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"
PCIE100DUALx.DeviceDesc   = "Intel(R) PRO/100 Dual Port Server Adapter"
PCIE100DUALSx.DeviceDesc  = "Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100S.DeviceDesc       = "Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc    = "Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc    = "Intel(R) PRO/100 S Server Adapter"

I559CMiniPCI.DeviceDesc   = "Intel(R) PRO/100+ MiniPCI"
MiniPCI3A.DeviceDesc      = "Intel(R) PRO/100+ MiniPCI Type 3A"
MiniPCI.DeviceDesc        = "Intel(R) PRO/100 P Mobile Adapter"
MiniPCIDes.DeviceDesc     = "Intel(R) PRO/100 SP Mobile Adapter"
MiniPCICombo.DeviceDesc   = "Intel(R) PRO/100 P Mobile Combo Adapter"
MiniPCIComboDes.DeviceDesc = "Intel(R) PRO/100 SP Mobile Combo Adapter"
MiniPCILON.DeviceDesc     = "Intel(R) PRO/100 Network Connection"

PCIE100BSPLUSD.DeviceDesc = "Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100S0.DeviceDesc       = "Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc       = "Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc    = "Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc    = "Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc      = "Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc      = "Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc    = "Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONLOM.DeviceDesc = "Intel(R) PRO/100 M Network Connection"
PCIE100LAVONMB.DeviceDesc  = "Intel(R) PRO/100 M Mobile Connection"
I559IFEAOLCPQ.DeviceDesc  = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

; Fujitsu Siemens Computers
Siemens558Wol.DeviceDesc= "Fujitsu Siemens Computers 82558-based Onboard Ethernet with WoL"
SiemensLan.DeviceDesc   = "Fujitsu Siemens Computers Server Onboard LAN with Intel 82558"
Siemens559Wol.DeviceDesc= "Fujitsu Siemens Computers 82559-based Onboard Ethernet with WoL"
SiemensWolAol.DeviceDesc= "Fujitsu Siemens Computers 82559-based Onboard Ethernet with WoL and AoL"
Siemens558.DeviceDesc   = "Fujitsu Siemens Computers Server Onboard LAN with Intel 82558"
Siemens559C.DeviceDesc  = "Fujitsu Siemens Computers Server Onboard LAN with Intel 82559C"

HPTX.DeviceDesc    = "HP NetServer 10/100TX PCI LAN Adapter"

IBMFE1.DeviceDesc  = "IBM 10/100 EtherJet PCI Adapter"
IBMFE2.DeviceDesc  = "IBM Netfinity 10/100 Ethernet Adapter"
IBMFE3.DeviceDesc  = "IBM 10/100 EtherJet PCI Management Adapter"
IBMFE4.DeviceDesc  = "IBM 10/100 EtherJet PCI Adapter with Alert on LAN"
IBMFE5.DeviceDesc  = "IBM 10/100 EtherJet Secure Management Adapter"
IBMFE6.DeviceDesc  = "IBM 10/100 EtherJet Secure Management Adapter"
IBMFE7.DeviceDesc  = "IBM Netfinity 10/100 Ethernet Security Adapter"
IBMFE8.DeviceDesc  = "IBM Netfinity 10/100 Ethernet Security Adapter"
IBMFE9.DeviceDesc  = "Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFEC.DeviceDesc  = "IBM 10/100 Ethernet Server Adapter"
IBMFED.DeviceDesc  = "Intel(R) PRO/100 S Network Connection"
IBMFEE.DeviceDesc  = "IBM 10/100 Dual Port Server Adapter"

PCIE100BSPLUSS.DeviceDesc = "Intel(R) PRO/100 S+ Server Adapter"
PCIE100SCBCOMBONODES.DeviceDesc = "Intel(R) PRO/100 Mobile Combo Adapter"
PCIE100SCBLANNODES.DeviceDesc   = "Intel(R) PRO/100 Mobile Adapter"
PCIE100SCBLANRNODES.DeviceDesc  = "Intel(R) PRO/100 R Mobile Adapter"
PCIE100SCBRCOMBONODES.DeviceDesc= "Intel(R) PRO/100 R Mobile Combo Adapter"

SamsungMiniPCI.DeviceDesc  = "Samsung SEM-2000 MiniPCI LAN Adapter"
SamsungILMiniPCI.DeviceDesc  = "Samsung SEM-2100iL MiniPCI LAN Adapter"
Toshiba82559B.DeviceDesc     = "Intel 8255x-based Fast Ethernet"

NEC82559BASED.DeviceDesc  = "NEC 82559-based Fast Ethernet Adapter"
PKUGX06.DeviceDesc        = "NEC PK-UG-X006(PCI) or compatible Fast Ethernet Adapter"
9821XB06.DeviceDesc       = "NEC PC-9821X-B06(PCI) or compatible/Intel 82557-based Ethernet"

; NT service name
e100bnt.Service.DispName = "Intel(R) PRO Adapter Driver"
